**LED BLINKING CODE:**

import RPi.GPIO as GP from time import

sleep

GP.setwarnings(False)

GP.setmode(GP.BOARD)

GP.setup(8,GP.OUT,initial=GP.LOW)

while True: #infinite loop GP.output(8, GPIO.HIGH)

# Turn on print(&quot;The LED is ON&quot;)

sleep(2) # Sleep for 2 second

GP.output(8, GPIO.LOW) # Turn off print(&quot;The LED is OFF&quot;)

sleep(2) # Sleep for 2 second

**TRAFFIC LIGHTRASBERRY:**

From gpiozero import LED

From time import sleep

Red= LED(17) #pin numbers connected to Led’s

Aster=(22)

Green=(27)

While True:

Red.on() #RED light

Print(“Red light is ON”)

For I in range(100,0,-1):

Print(“Remaining time: “,i)

Sleep(1)

Red.off()

Aster.on() # ASTER light

Print(“Yellow light is ON”)

For I in range(5,0,-1):

Print(“Remaining time: “,i)

Sleep(1)

Aster.off()

Green.on #GREEN light

Print(“Green light is ON”)

For I in range(30,0,-1):

Print(“Remaining time: “,i)

Sleep(1)

Green.off()